{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet 1","index":0,"n_rows":9,"n_cols":8,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
["NOUN","MODIFIER","NM_Abbrivation","Attribute","Attribute Definition","Mandatory","Short Sequence","Long Sequence"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","TYPE","USE EITHER A GENERIC VALUE THAT SPECIFICALLY NAMES THE TYPE, OR DEFAULT TO AN APPLICATION VALUE OF THE CLOSEST PIECE OF EQUIPMENT. GENERALLY, THIS EXCLUDES BRAND NAMES OR MANUFACTURER TYPES USED TO DESCRIBE THEIR PRODUCTS.","MANDATORY",null,"1"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","MATERIAL","WHEN KNOWN, ENTER PROCESS, PLATING, BASE MATERIAL, MATERIAL SPECIFICATION AND GRADE. FOR STAINLESS STEEL PRECEDE SS WITH THE AISI GRADE.","MANDATORY",null,"2"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","MATERIAL SPECIFICATION","TO BE SATISFIED BY AB MATERIAL, DESIGN, PRODUCT, OR SERVICE","OPTIONAL",null,"3"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","PRESSURE RATING","ENTER THE PRESSURE RATING OF THE ADAPTER","OPTIONAL",null,"4"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","TUBING CONNECTION","ENTER THE TUBING CONNECTION OF THE ADAPTER","MANDATORY",null,"5"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","PIPE CONNECTION","ENTER THE TYPE OF PIPE CONNECTION. ENTER THREAD SIZES ONLY IF DIFFERENT FROM NOMINAL SIZE. ENTER SCREW(ED) AS THD.","MANDATORY",null,"6"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","TUBING SIZE","ENTER THE SIZE OF THE TUBING WHICH IS TO BE SWABBED.","MANDATORY",null,"7"]
["ADAPTER","TUBE TO PIPE","ADAPTER,TUBE TO PIPE","PIPE SIZE","ENTER THE NOMINAL SIZE OF THE PIPE ONLY. IF ONLY ONE SIZE IN DESCRIPTION, ENTER SIZE IN BOTH TUBE SIZE AND PIPE SIZE.","MANDATORY",null,"8"]