{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet 1","index":0,"n_rows":3,"n_cols":7,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["Itemcode","Material code","Mat Description","Basic Data Text","Purchase Order Text","Shortdesc","Longdesc"]
["CEM1010473","5100017774","1 1/2\"ELBOW 45°CS SMLS SCH20 A234 GRWPB","1 1/2\"45 DEG. ELBOW, CS, SEAMLESS, SCH 20, BEVELLED ENDS, R = 1.5D, ASTM  A 234 GR. WPB SEAMLESS, ASME B 16.9 COG","SPARES","ELBOW PIPE,BE,B16.9,CS,ASTM  A234 GR WPB","ELBOW,PIPE,END CONNECTION:BEVELLED END,DIMENSIONAL SPEC PIPE:ASME B16.9,MATERIAL:CARBON STEEL,MATERIAL SPECIFICATION:ASTM  A234 GR WPB,MANUFACTURING PROCESS:SEAMLESS,ANGLE:45 DEG,RADIUS:1.5D,SCHEDULE NUMBER:SCH 20,SIZE:1-1/2 IN,ADDITIONAL INFORMATION:COG"]
["CEM1038178","4100002362","1\" CPVC ELBOW","--","CONSUMABLES","ELBOW PIPE,CPVC,1IN","ELBOW,PIPE,MATERIAL:CHLORINATED POLYVINYL CHLORIDE,SIZE:1 IN"]