{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet 1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet 1","index":0,"n_rows":3,"n_cols":25,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["EQUIPMENT NUMBER","EQUIPMENT TAG","EQUIPMENT DESCRIPTION","EQUIPMENT INDICATOR","MATERIAL GROUP","MATERIAL CRITICALITY","MATERIAL #","MATERIAL SHORT DESCRIPTION","MATERIAL LONG DESCRIPTION","MANUFACTURER","MODEL NUMBER","PART NUMBER","SERIAL NUMBER","DRAWING NUMBER","MANUFACTURER (OCM)","PART NUMBER (OCM)","ITEM CATEGORY","UNIT OF MEASURE","INSTALLED QTY","RECOMMENDED QTY (SPIR/PSPL/SPL)","INITIAL MRP (MIN)","INITIAL MRP (MAX)","REMARKS","FILE NO","PAGE"]
["5128008","A02-PT-21024A","PT21024A U2101 PRESSURE TRNS","A","41112410","VITAL","NEW CODE_5000068","TRANSMITTER,PR,-1TO80BARG,266PSHQS8A2A8","TRANSMITTER, PRESSURE, TYPE: SMART, RANGE: -1 TO 80 BARG, OUTPUT: 4-20MA HART, SENSOR TYPE: INDUCTIVE, PROCESS CONNECTION SIZE: 1/2 IN FNPT, ELECTRICAL CONNECTION SIZE: 2 X 1/2 IN FNPT, BODY MATERIAL: SS 316L, MOUNTING: 2 IN PIPE MOUNT, WITH COMPLETE MANIFOLD VALVE MODEL NUMBER: M26DAS2VSGGF16SN2, MANUFACTURER: ABB, MODEL NUMBER: 266PSHQS8A2A8-E9L1I2H3A1","ABB","266PSHQS8A2A8-E9L1I2H3A1",{"$nulls":5},"INSTRUMENTATION","EA","1",null,"1","1",null,"JIGCC-A00-QC-VIR-00663[00].ZIP.11A\\DOC-0073137-00\\A00-ZA-E-0073137_00.PDF","2512"]
["5128011","A02-PT-21024B","PT21024B U2101 PRESSURE TRNS","A","41112410","VITAL","NEW CODE_5000068","TRANSMITTER,PR,-1TO80BARG,266PSHQS8A2A8","TRANSMITTER, PRESSURE, TYPE: SMART, RANGE: -1 TO 80 BARG, OUTPUT: 4-20MA HART, SENSOR TYPE: INDUCTIVE, PROCESS CONNECTION SIZE: 1/2 IN FNPT, ELECTRICAL CONNECTION SIZE: 2 X 1/2 IN FNPT, BODY MATERIAL: SS 316L, MOUNTING: 2 IN PIPE MOUNT, WITH COMPLETE MANIFOLD VALVE MODEL NUMBER: M26DAS2VSGGF16SN2, MANUFACTURER: ABB, MODEL NUMBER: 266PSHQS8A2A8-E9L1I2H3A1","ABB","266PSHQS8A2A8-E9L1I2H3A1",{"$nulls":5},"INSTRUMENTATION","EA","1",null,"1","1",null,"JIGCC-A00-QC-VIR-00663[00].ZIP.11A\\DOC-0073137-00\\A00-ZA-E-0073137_00.PDF","2513"]